CANOPY POSITIONING

TIP: HAVE ONE PERSON ON EACH SIDE OF THE LO PRO TO MOVE THE CANOPY TOGETHER

HOW TO LAY THE CANOPY FOR TRAILERING

* The canopy frame arms should be in the front and rear brackets
* Push the canopy from the front bow back until it lays down completely
* Secure the canopy by taping to the siderail

HOW TO OPEN THE CANOPY

* Make sure the canopy frame arms are the rear and middle brackets
* Take off the boot by unzipping it from the canopy
* Grab the front bow and pull it forward until the canopy is completely open
* Hook the straps from the front bow loop to the loop that is on the siderail by the front bracket
* Tighten the straps to create tension by pulling the front bow forward slightly

HOW TO CLOSE THE CANOPY

* The canopy frame arms should be in the middle and rear brackets
* Unhook the straps from the siderail loop
* Push the front bow back until the canopy is folded up
* Put the boot back on the canopy and zip it up